Title: Schüco AWS 75
Author: ropelt
Last saved by: Mrugalla, Daniel
Company: Schueco International KG

Schüco AWS 75.SI+, highly thermally insulated aluminium window system 
With 75 mm basic depth.

Design features:
Face-fitted vent frame on the room side rebated by 10 mm from the frame edge, flush-fitted on the outside.
Thermally insulated insulating bars with three hollow chambers form the rebate for the co-extruded, double hollow chamber centre gasket fitted with a foam core. 
The system must be fitted with square glazing beads. 
The glazing beads are installed with plastic clips to compensate tolerances.

Profile basic depths:
Outer frame, mullion, transom	75 mm
Vent frame	85 mm

Profile face widths:
Outer frame, bottom	104 mm
Outer frame, side and top	79 mm
Insert outer frame	44 mm
Mullion	94 mm
Transom	94 mm
Vent frame (window)	41 mm
Vent frame (window door)	51 mm
Double-vent profile	67 mm