Title: Schüco AWS 90
Author: ropelt
Company: Schueco International KG

Schüco AWS 90.SI+, aluminium window system to passive house standard 
With 90 mm basic depth.

Design features:
Face-fitted vent frame on the room side rebated by 10 mm from the frame edge, flush-fitted on the outside.
Thermally insulated insulating bars with three hollow chambers in the vent and foam insulation form the rebate for the co-extruded, hollow multi-chamber centre gasket, which is fitted with a foam core and has three fins to reduce convection. 
The centre gasket is attached in the area of the insulation zone to the insulating bars by means of a double locating groove and hooking in at the rear.
The glazing rebate is thermally insulated by means of foam profiles which are tailored to the profile system and wrap around the outer insulating glass edge. 
The system must be fitted with square glazing beads. 
The glazing beads are installed with plastic clips to compensate tolerances.

Profile basic depths:
Outer frame, mullion, transom	90 mm
Vent frame	100 mm

Profile face widths:
Outer frame, bottom	109 mm
Outer frame, side and top	84 mm
Mullion	104 mm
Transom	104 mm
Vent frame (window)	36 mm
Vent frame (window door)	46 mm
Double-vent profile, narrow	62 mm