Author: ropelt
Company: Schueco International KG

Schüco AWS 50, thermally insulated aluminium window system
With 50 mm basic depth.

Design features:
Face-fitted vent frame on the room side rebated by 10 mm from the frame edge, flush-fitted on the outside.
The system must be fitted with square glazing beads.
The glazing beads are installed with plastic clips to compensate tolerances.

Profile depths:
Outer frame, mullion, transom	50 mm	
Leaf frame	60 mm
Vent frame, Top Swing	75 mm

Profile face widths:
Outer frame, bottom	94 mm
Outer frame, side and top	79 mm
Mullion	94 mm
Transom	94 mm
Vent frame (window)	41 mm
Vent frame (window door)	61 mm
Double-vent profile (window)	52 mm