Title: Schüco ADS 70
Author: ropelt
Company: Schueco International KG

Schüco ADS 70.HI, highly thermally insulated aluminium door system 
With 70 mm basic depth.

Design features:
Internal and external flush-fitted door constructions with 5 mm shadow joint on both sides; with 11 mm shadow joint for double-leaf panic doors.
The thermal breaking split insulating bars are fitted with foam insulation for high thermal insulation.
The door leaf profiles are fitted with thermal breaking split insulating bars.
The door leaves must have a four-sided mitre-cut leaf profile.
The system must be fitted with square glazing beads. 
For increased thermal insulation, glazing gaskets with fins must be used.
If there are no other requirements specified for the sill by standards / guidelines / local building regulations, the bottom door sill must be fitted with an aluminium/plastic rebate threshold, height 20 mm, and a gasket system for sealing at a test pressure of up to 150 PA in accordance with DIN EN 12208.

Profile basic depths:
Outer frame, mullion, transom	70 mm
Leaf frame (door), flush-fitted	70 mm
Leaf frame (door) with internal rebate	80 mm

Profile face widths:
Outer frame / sill, bottom	106 mm
Outer frame, side and top	79 mm
Mullion	94 mm
Transom	94 mm
Inward-opening leaf frame,
flush-fitted inside and outside,
continuous	73 mm
Outward-opening leaf frame,
flush-fitted inside and outside,
continuous	98 mm
Leaf frame 
(Door, with internal rebate)	73 mm
Meeting stile profile	65 mm
Leaf mid-rail	94 mm